CLI COMMANDS

STATIC-

enable

conf t

ip route ip subnet next hop

exit

wr

RIP-

enable

conf t

router rip

network “ ip”

network two

settings save

DHCP-

en

conf t

int fa 0/0

ip address ip subnet

no shutdown

do write memory

ip dhcp pool net1

network ip subnet

repeat for net2 and all

select dhcp

OSPF-

enable

configure terminal

interface serial 2/0

ip address ip subnet

clock rate 72000

no shutdown

interface fastethernet 0/0

ip address ip subnet

no shutdown

exit

router ospf1

network ip 0.0.0.255 area 0

network ip 0.0.0.255 area 0

exit

save in settings

FTP-

Save a file

Go to services ftp username pass

ping server ip

ftp server ip

enter all dets

put hello.txt

dir

in 2nd pc- ftp server ip

dets

get hello.txt